Jump to main content

# Software and hardware requirements

Minimum requirements:

- personal computer: Pentium 1 Ghz processor, RAM – 1024 Mb, free disk space – 10 GB;
- OS: Microsoft Windows (x32/x64) 8/8.1/10/11;
- OS:Windows Server (x64) 2008 R2/2012 R2/2016.

Important: If cryptographic service providers, which implement GOST cryptographic algorithms, produced by other manufacturers have been already installed on the computer, the ТУМАР-CSP software correct operation cannot be guaranteed due to the Windows OS architecture peculiarities.

Security tokens

The following table provides information about the supported security tokens, depending on the «ТУМАР-CSP» software version.

Name | v.6.2 | v.6.3 | v.6.4
file system | + | + | +
the «JaCarta electronic key» family (USB/SmartCard) | + | + | +
electronic USB-key eToken PRO 32K (USB) | + |  |
electronic USB-key eToken PRO 72K (Java) (USB/SmartCard) | + | + | +
electronic identifier KAZTOKEN (USB/SmartCard) | + | + | +
GemPlus, device produced by Gemalto (SmartCard) | + |  |
SafeNet eToken 5110 (USB/SmartCard) | + | + | +

Using plug-ins

The following table contains information about supported plugins depending on the «ТУМАР-CSP» software version

Name | Destiny | v.6.2 | v.6.3 | v.6.4
DigiFlow LLP. & Aladdin Token JC & ARDS JaCarta | to work with eToken PRO 72K /JaCarta/KAZTOKEN/SafeNet eToken 5110 devices | + | + | +
New algorithm for tokens | to work with eToken PRO 72K/JaCarta and key information using object identifiers (OIDs) of the Republic of Kazakhstan | + | + | +
jaCarta Laser | to work with JaCarta devices | + | + | +
jToken Key Store | to work with eToken PRO 32 K devices | + |  |
Aladdin Token & BCC | to work with eToken PRO 72K/JaCarta devices | + |  |
GemPlus Key Store | to work with «GemPlus» devices | + |  |

Random number generators

The following table contains information about supported random number generators, depending on the «ТУМАР-CSP» software version.

Name | Type 1 | v.6.2 | v.6.3 | v.6.4
Software generator | Biometric | + |  |
eToken PRO 72K/JaCarta (USB/SmartCard) | Hardware |  | + | +
JaCarta (USB/SmartCard) | Hardware |  | + | +
SafeNet eToken 5110 (USB/SmartCard) | Hardware |  | + | +

TUMAR-CSP software working jointly with anti-virus programs:

Before installing the «ТУМАР-CSP» software it is recommended to disable the anti-virus program.

1. In order to operate the Kaspersky Anti-Virus software correctly, the following program installation sequence is recommended:
   - install the Kaspersky Anti-Virus software;
   - install the «ТУМАР-CSP» software.
2. Correct operating the McAfee anti-virus program is possible when you first disable the Buffer overflow protection option in its settings, then install the «ТУМАР-CSP» software on the workstation.
3. For the correct installation of the «ТУМАР-CSP» software on the workstation with the current Dr.Web Security Space software version already installed, it is necessary to activate the Preventive Protection mode of the Dr.Web Security Space software and enable the Windows shell autorun. In order to do this:
   - click on the Software icon located in the systray with the right mouse button to open the context menu. Select the Tools menu Item > Settings;
   - click on the Settings > Basic and switch over to the Preventive protection tab, then click on the User button in the window working area;
   - click on Allow the Windows shell autorun option in the Preventive protection window;
   - accept the changes made to the Dr.Web Security Space software settings;
   - install the «ТУМАР-CSP» software on the workstation.
4. Correct interaction between the «ТУМАР-CSP» software and SWIFT Alliance software is possible when the TUMAR-CSP software is installed in succession to the SWIFT Alliance software installation and if the SWIFT Alliance core process is activated.

When installing the SWIFT Alliance software on a computer where the «ТУМАР-CSP» software has already been installed, it is required:

- to uninstall the «ТУМАР-CSP» software;
- to install, configure and run the SWIFT Alliance software;
- to install the «ТУМАР-CSP» software.

1 Support for hardware random number generator is determined by customer requirements.